Analysis Report

|  |
| --- |
| **Project: Prevention of alleyway accidents with MOG2 algorithm and GIS analysis.** |
| **The Details** |

**◦** Analysis overview

|  |  |
| --- | --- |
| |  | | --- | | **1. Background and Necessity**  A traffic accident is any case that creates a traffic hazard. The social cost of traffic accidents is estimated at 32 billion USD a year in South Korea.  According to data released by the Seoul Metropolitan Police Agency, Gangseo-gu(district in Seoul) and Gangnam-gu(district in Seoul) are known to have the most frequent traffic fatalities among 25 autonomous districts in Seoul in 2020. It is expected that the increase in traffic accidents on residential roads due to the recent increase in traffic volume on residential roads due to the recommendation of detour routes by navigation has had an impact on the increase in traffic accidents. According to the ‘2017 Traffic Statistics of the Korea Machinery Industry Promotion Association’, the number of fatalities in traffic accidents occurring on living roads reached 57%.  To make Gangseo-gu(district in Seoul) safe from traffic accidents, we analyze the causes of traffic accidents in Gangseo-gu(district in Seoul) and propose solutions to reduce traffic accidents based on this.  **2. Analysis purpose**  When driving a vehicle on a road(alleyway intersection) where visibility is not secured, the existing security CCTV camera on the road will notify/warn driver or surrounding with lighting if there’s another car/human is coming across from side of the intersection. Security CCTV camera analyze movement, and based on this, a warning light on the CCTV camera will light up prevent accidents occurring at intersections and living roads. The purpose of this analysis is to solve the traffic accident problem.  In order to understand the causes of traffic accidents in Gangseo-gu, indicators and locations related to traffic accidents that occurred in Gangseo-gu from 2016 to 2020 were analyzed. As a result of the analysis, it was confirmed that many traffic accidents occurred at alleyway intersections. In order to solve this problem, we propose an alternative for securing the driver's field of vision on the road through data analysis, and expect to reduce traffic accidents and reduce social costs in Gangseo-gu through this. | |

|  |
| --- |
| ◦ Analysis result details |
| |  | | --- | | **1. Analysis data and analysis tools**  A. Traffic Accidents in Gangseo-gu   1. Utilization of 'TAAS Traffic Accident Analysis System' traffic data 2. Period of collected data: 2016-2020 3. Details and location (coordinates) data of traffic accidents that occurred in Gangseo-gu 4. The accident situation corresponding to the accident is recorded in detail 5. EDA data with pandas and geopandas libraries and write the coordinates in the data in a form usable to the pydeck library   B. Population density of Gangseo-gu   1. From 'Seoul Open Data Plaza' we used Seoul population density statistics 2. The latest data currently provided (20 years) 3. Population density is the number of people per area (1 km²) 4. The data records the population and area of ​​each administrative dong registered by 20 years and provides the obtained population density   \* For the public data used in the analysis, the latest accessible version was used.  **2. Algorithm**  A. Geographic Information System (GIS)  We identified the trend of traffic accidents in Gangseo-gu, and analyzed the accident rate and population density. In this process, a GIS that can visually emphasize the relationship between traffic accidents and population density was adopted.  GIS modeling provides various types of information necessary for decision-making by finding hidden patterns and relationships in spatial phenomena. Based on this, it is an analysis method that derives solutions and predicts changes in space.  By integrating and managing location data and attribute data for objects with geographic locations, it is possible to identify problems based on analysis of inter-information such as maps and diagrams, and to derive various insights of space by grasping predictions and trends.  B. MOG (Mixture of Gaussian)  MOG is one of the algorithms that removes the background in real time in the process of image analysis and is very effective and often used. The MOG algorithm based on the Gaussian mixture model sets a probabilistic model for each pixel in the image to distinguish objects in the background and foreground. We chose the MOG2 algorithm based on the Gaussian mixture model to remove the static background and track the motion of an object as a method for analyzing CCTV images.    [Figure 1] Object Recognition Flowchart  MOG2 is a model that will develop the Gaussian distribution of MOG, has excellent background and foreground segmentation performance, and shows high adaptability in various environments where light changes occur. In addition, since shadow detection is possible, there is an advantage in that objects can be accurately distinguished. In the image analysis process, the MOG2 algorithm was used to compare the current and previous frames as shown in [Figure 1], remove the static part, extract only the part where the change occurred and express it in white, and use the outline for the part expressed in white. This increases the recognition rate of objects.  object recognition sequence   1. Sequentially extract images from video frames. 2. After changing the extracted image to a black-and-white image to improve performance, set the desired detection section. 3. Using MOG2, remove the static background to black and remove the moving object and extracted to white. 4. Emphasizing necessary objects through the closing technique and preventing noise expansion at the same time. 5. Through the opening technique, the object is protected as much as possible, and noise is removed. 6. The recognition rate is increased by applying the dilation calculation twice to highlight the object. 7. When recognized object is entering the detection area after creating a green outline on the recognized object, warning signal show up on the screen.   3. Analysis Methodology  A. planning stage   1. Contribute to improving the welfare of residents using Gangseo-gu public data 2. Check CCTV location and illegal parking location data for peace of mind among public data   - Hypothesis: increase in traffic accidents due to increase in illegal parking  - Proposal: To reduce traffic accidents, provide an alternative using CCTV for relief  B. data preparation   1. Collecting public data such as public data portal and Seoul public data 2. TAAS data collection for data collection on traffic accidents   C. data analysis   1. Pre-process (EDA) TAAS data and analyze associations for each variable 2. Finding meaningful data 3. Additional data collection based on analysis results 4. (Administrative-dong boundary, Gangseo-gu population, CCTV video data, etc.) 5. Repeat the preparation and analysis steps to the desired level   - Visualize preprocessing (EDA) data  - Analyze visualization data  - Check the basis for the hypothesis  D. system implementation   * 1. Start constructing a model to realize our team's proposals for the hypothesis   2. Build the desired model through the background removal algorithm with the collected image data   E. Model evaluation and analysis   1. Confirmation and verification of proposals | |

|  |
| --- |
| **◦ Results and implications** |
| |  | | --- | | 1. Results and Insight    [Figure 2] Gangseo-gu Traffic Accident Area and Population Density by Dong(District)  Based on the TAAS data on traffic accidents in Gangseo-gu and the population density of Gangseo-gu, the GIS analysis was used to visualize the distribution of traffic accidents and the population density of each administrative dong as shown in [Figure 2] to analyze the correlation. In the case of traffic accidents, the data were analyzed by dividing it into two types: ‘car-to-car’ and ‘car-to-car’.    [Figure 3] Total Number of Accidents by Dong(District) in Gangseo-gu  As shown in [Figure 3], the administrative dong with the highest number of traffic accidents in Gangseo-gu from 2016 to 2020 was Hwagok 1-dong, followed by Gayang 1-dong and Banghwa 2-dong. As a result of analyzing the graph in terms of the relationship between population density and traffic accidents, the highest number of traffic accidents occurred in Hwagok 1-dong, a residential area with high population density.    [Figure 5] Number of vehicle-to-person accidents by dong    [Figure 6] Number of vehicle-to-vehicle accidents by dong  Looking at the trend of traffic accidents that occurred in Gayang 1-dong and Banghwa 2-dong, which have low population density, as shown in [Figure 5], the number of traffic accidents by vehicle person is in the low-middle range, whereas [Figure 6] It can be seen that the car accident occurrence ranking is in the 1st and 3rd places.  As a result of these environmental factors, it can be seen that Hwagok 1-dong, which has the highest population density, recorded a higher total number of traffic accidents than Gayang 1-dong and Banghwa 2-dong. The higher the population density, the higher the ratio of car-to-person traffic accidents on living roads, and the lower the population density, the fewer traffic accidents on the living roads.  Analyzing the causes of accidents in Hwagok 1-dong, which has a high population density, as shown in [Figure 1], it can be visually confirmed that most of the traffic accidents occur on living roads. In addition, In [Figure 7], it can be seen that non-compliance with safe driving accounts for the highest proportion of 66.8% among the causes of traffic accidents in Hwagok 1-dong.  [Figure 7] Causes of traffic accidents in Hwagok 1-dong  Due to the characteristics of Hwagok-dong, which has a high population density and many housing complexes, drivers have difficulty in securing visibility due to illegally parked and parked vehicles on the road. In addition, it can be predicted that many drivers are careless while driving on the road and cause traffic accidents due to the causes of traffic accidents.  We are going to propose a road keeper safety system that utilizes CCTV footage to reduce traffic accidents occurring on living roads. For image analysis, the recognition rate was improved by reducing the distribution curve of a stationary object based on the analysis of the MOG2 model of OpenCV and lowering the recognition rate by increasing the distribution curve of a moving object. The goal is to prepare for movement that occurs in the driver's blind spot by turning on a warning light when a car or person moves within a specified distance. | |
| **◦ Utilization plan and expected effect** |
| |  | | --- | | 1. Utilization sector  One of the biggest causes of traffic accidents is the driver's blind spot. If you check the result of GIS analysis of traffic accident data, you can see that a lot of traffic accidents occur not only on the roadside where there are many vehicles, but also at intersections and daily roads where the driver's line of sight is not secured.  Assuming a traffic accident situation occurring at an intersection of an alleyway, it is difficult for drivers and pedestrians to immediately recognize the situation on the left and right sides of the road straight ahead due to blind spots of view. From the driver's point of view, a traffic accident may occur due to a vehicle or pedestrian suddenly appearing from the blind spot. As a way to solve this problem, we devised a road keeper notification system that recognizes the movement of pedestrians and vehicles in the driver's blind spot based on AI analysis and notifies the driver of the risk of an accident through a warning light.  Relief installed in road intersection areas such as crossroads or three-way intersections, which are frequent traffic accident sections, analyzes the movement of objects and people in the CCTV video data by AI analysis to ensure that vehicles or pedestrians entering from the right or left side of the driver are detected at the intersection. When approaching within a certain distance, a warning light is turned on.  2. Expected effect  The road keeper notification system provides information about blind spots in the front sight by installing a warning light that can notify the driver or pedestrian of the surrounding situation when a movement of an object is confirmed based on the result of analyzing the image.  Through this, it is expected that it will be possible to reduce the incidence of accidents in the alley intersection section by giving drivers attention to the accident situation in advance and recognizing the causes of the accident.  Another expected effect is cost reduction. The existing relief installed in Gangseo-gu is expected to reduce the cost of installing the system by analyzing the CCTV images through MOG2 analysis system. [Figure 7] shows that the recognition range based on the location of the security camera (●) and the area where the traffic accident occurred (●) overlap.    [Figure 7] The intersection range of the traffic accident area and the safety CCTV  In addition, it can be used in various ways not only in alleys and living roads with many parking lots, but also in places where visibility is difficult, such as alleys entering the roadside. If Hwagok-dong, which has a high population density and many roads for living, is selected as a pilot area, the effectiveness of the road guard system by MOG2 algorithm can be identified within a short period of time. | |

|  |
| --- |
| **◦ Sources of utilization data and references** |
| |  | | --- | | **1. Public data**   1. TAAS, Traffic Accident Analysis System, <http://taas.koroad.or.kr> 2. Statistical geographic information service, administrative dong boundary data of Korea, <https://sgis.kostat.go.kr/view/index> 3. Seoul Open Data Plaza, Seoul population density (by dong) statistics, <https://data.seoul.go.kr/dataList/10584/S/2/datasetView.do> 4. Public data portal, CCTV installation status in Seoul, https://www.data.go.kr/data/15081885/fileData.do   **2. References**   1. Road Traffic Authority, Analysis of Traffic Accident Factors, 2014 2. Road Traffic Authority, Statistical Analysis of Traffic Accidents in 2021 Edition, 2021 3. Seok-Bin Song, Jin-Heon Kim, SFMOG MOG: A paper on an ultra-fast-based background removal algorithm, 2019 4. Hyejin Kim, CNN image analysis for distance measurement and lidar point cloud-based object recognition and visualization, Master's thesis, Hanyang University, 2018 5. Chul-Woo Jeong, A Study on the Influencing Factors of Drowsy Driving through Binary Logistic Regression, Public Security Policy Institute, 2006 6. Kim Young-pyo, Lim Eun-sun, GIS-based spatial analysis method application study, 2004 7. Maeil Economic Daily, 43 trillion won in social costs due to road traffic accidents… 2.3% of GDP, https://www.mk.co.kr/news/economy/view/2021/04/334377/ 8. The Kyunghyang Shinmun, 70% of pedestrian traffic fatalities in Seoul were caused by pedestrian negligence. Gangseo-gu and Gangnam-gu ranked first in traffic accident deaths https://www.khan.co.kr/national/incident/article/202102071200001 9. Yonhap News, "Cars running in our neighborhood…Is the alleyway a highway? https://www.yna.co.kr/view/AKR20180202182800797 | |